[bookmark: _Hlk194381393]PTWL 02 - Permit to Work Inspection Checklist
Macro QHSEW team and Facility Managers shall complete this inspection checklist for PTW issued by Macro and/or Suppliers competent staff to Macro or Suppliers works.
	Site: 
	
	Permit No: 	Comment by Barbara Gallani: In thi s box we can add : Risk Category Level: ☐ Level 1 ☐ Level 2.A (Remote) ☐ Level 2.B (On-site) | | Supervision Required: ☐ Remote ☐ On-site Dynamic Risk Assessment completed? ☐ Yes ☐ No (attach evidence) |	Comment by Levente Marton: L1 is low risk, not require PTW.
	

	Work Activity: 
	
	Permit Type: 
	

	
             Permit issued by Macro or Supplier:  _______________________     Inspection done by Macro(name):
                                                                                                                                              
                                                                                 

	No.
	Description
	Y/N/NA
	Remarks 
(include evidence seen if done remotely)

	1
	Is the correct PTW is issued for the scope of work?
	
	

	2
	Are PTW signed by person authorizing and accepting the work?
	
	

	3
	Is the PTW issuer competent and NOT part of the work team?
	
	

	4
	Is the work within the date and time limit on the PTW?
	
	

	5
	Is the work being carried out as written in the PTW and the associated RAMS/JHA? Are all preventive measures implemented?
	
	

	6
	4a  Are all preventive/control measures implemented before work starts?
4b  Are all control measures maintained and effective throughout the task?
	
	

	7
	Are Method Statement & Risk Assessment attached to PTW? Is the PTW posted visibly at work locations?
	
	

	8
	Are workers received Site Induction?
	
	

	9
	Has the induction been completed within the validity period (site or project-specific)?
	
	

	10
	Has worker competence been verified through certificates/logbooks?
	
	

	11
	Are workers briefed on Risks and Method Statement and other specific measures agreed in the PTW?
	
	

	12
	Are the PPEs appropriate for the task and are used?
	
	

	13
	Is special PPE required (arc flash, chemical, rope access) and is it valid/in-date?
	
	

	14
	Are warning tags/caution notices and barricades(cordoned) provided?
	
	

	15
	Are barriers appropriate for risk level (e.g., rigid barriers for high-risk areas)?
	
	

	16
	Are Tools and Equipment suitable and in good condition?
	
	

	17
	Are third-party inspection certificates available where required (MEWP, lifting, scaffolding)?
	
	

	18
	Are SDS for hazardous chemicals available?
	
	

	19
	“SDS < 5 years old and site-specific to chemical brand?”
	
	

	High risk PTW specific questions
To be completed if is applicable, not all sections are mandatory.


	
Precautions For Hot work

	
	Y
	N
	N/A
	
	Y
	N
	N/A

	Are combustible waste materials removed from work area?
	|_|
	|_|
	|_|
	Is Fire Watch available?
	|_|
	|_|
	|_|

	Is local exhaust ventilation installed to remove toxic content and disperse smoke?
	|_|
	|_|
	|_|
	Is the welder competent?
	|_|
	|_|
	|_|

	Hot Work Permit displayed at site.”
	
	
	
	Flammable gases detected? Gas monitoring performed?”
	
	
	

	Are all walls and floor openings covered or protected?
	|_|
	|_|
	|_|
	Are smoke detectors covered or decommissioned to prevent false alarms?
	|_|
	|_|
	|_|

	“Fire watch duration after work completed (min. 30–60 min depending on local law).”
	
	
	
	
	
	
	

	Are welding screens used?
	|_|
	|_|
	|_|
	Fire extinguisher
	DCP |_|
	CO2 |_|
	Water |_|
	Foam |_|


	Precautionary Measures for Confined Space

	
	Y
	N
	N/A
	
	Y
	N
	N/A

	Is Emergency Rescue Plan in place? Is the Stand-by Person present? Is communication system in place?
	|_|
	|_|
	|_|
	Are electricity and other energy sources isolated? Is LOTO applied?
	|_|
	|_|
	|_|

	Are safe entry and egress provided?
	|_|
	|_|
	|_|
	Are equipment drained/emptied and isolated?
	|_|
	|_|
	|_|

	Entry permit issued?”
	
	
	
	Last atmospheric test timestamp + values recorded.”
	
	
	

	All entrants listed and signed onto permit.”
	
	
	
	
	
	
	

	Is the rescue lifting tripod available on site?
	|_|
	|_|
	|_|
	Is forced ventilation available and operable?
	|_|
	|_|
	|_|

	Is calibration of Air Sampling Device valid? Are air samplings being done at regular frequency?
	|_|
	|_|
	|_|
	Is Adequate lighting not exceeding 110V implemented?
	|_|
	|_|
	|_|


	[bookmark: _Hlk188787627]Precautionary Measures for Rope Access Work

	
	Y
	N
	N/A
	
	Y
	N
	N/A

	Is Emergency Rescue Plan in place?
	|_|
	|_|
	|_|
	Is communication system in place?
	|_|
	|_|
	|_|

	Are Rope Access Team members competent/certified to do the work (IRATA Level-1 Technician & Level-3 Supervisor)?
	|_|
	|_|
	|_|
	Is wind Monitoring being carried out?
	|_|
	|_|
	|_|

	Is calibration of Anemometer valid?
	|_|
	|_|
	|_|
	Is third party inspection valid for PPE Kit? Is third party inspection valid for anchor point?
	|_|
	|_|
	|_|


	Precautionary Measures for Working at Height

	
	Y
	N
	N/A
	
	Y
	N
	N/A

	Is wind Monitoring being carried out?
	|_|
	|_|
	|_|
	Is Scaffolding Inspected and Tag  provided?
	|_|
	|_|
	|_|

	Are there any  hazards  present in the vicinity?
	|_|
	|_|
	|_|
	Is the Safety harness attached to anchor point?
	|_|
	|_|
	|_|

	Is the Safety harness inspected/
	|_|
	|_|
	|_|
	Is the Anchor point third party inspected?
	|_|
	|_|
	|_|

	Is the MEWP/BMU third party inspected?
	|_|
	|_|
	|_|
	Are tools and equipment properly tethered?
	|_|
	|_|
	|_|

	Fall protection rescue kit available & workers trained to use it.”
	
	
	
	
	
	
	

	Precautionary Measures for Electrical works

	
	Y
	N
	N/A
	
	Y
	N
	N/A

	Is electrical energy isolated and LOTO applied?
	|_|
	|_|
	|_|
	Are the adjacent active parts of the electrical installations are covered with insulating materials?
	|_|
	|_|
	|_|

	“Isolation point correctly labelled and secured?”
	
	
	
	Shock/arc flash boundaries set and marked?”
	
	
	

	Is the presence of electrical power tested after LOTO applied?
	|_|
	|_|
	|_|
	Is Third party inspection valid for PPE Kit?
	|_|
	|_|
	|_|

	Voltage testing equipment calibrated?”
	
	
	
	
	
	
	

	Is specific electrical PPE used according to arc flash requirements?
	|_|
	|_|
	|_|
	Is Arc flash study done for PPE required?
	|_|
	|_|
	|_|


	Precautionary Measures for Lifting activities

	
	Y
	N
	N/A
	
	Y
	N
	N/A

	Is the lifting plan prepared and followed?
	|_|
	|_|
	|_|
	Is communication system in place?
	|_|
	|_|
	|_|

	“Lift plan signed by Appointed Person.”
	
	
	
	Tag lines used where appropriate.”
	
	
	

	Is Emergency Rescue Plan available?
	|_|
	|_|
	|_|
	 Are all rigging inspected and marked?
	|_|
	|_|
	|_|

	Are the lifting equipment  inspected a maintained according to local legal requirements?
	|_|
	|_|
	|_|
	Is wind monitoring being carried out?
	|_|
	|_|
	|_|

	Is area free of any overhead obstructions?
	|_|
	|_|
	|_|
	Are all hooks provided with functional safety latch?
	|_|
	|_|
	|_|

	Precautionary Measures for Excavations

	
	Y
	N
	N/A
	
	Y
	N
	N/A

	Is Emergency Rescue Plan in place? Is Communication System in place?
	|_|
	|_|
	|_|
	Is electrical cable detection devices available?
	|_|
	|_|
	|_|

	Are underground schemes available and checked?
	|_|
	|_|
	|_|
	Is pipeline detection available?
	|_|
	|_|
	|_|

	Are underground networks signalised and visible?
	|_|
	|_|
	|_|
	Is trained banksman allocated?
	|_|
	|_|
	|_|

	Shoring/benching in place where required?”
	
	
	
	Edge protection around excavation?”
	
	
	

	Excavation inspections performed daily?”
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	


	Inspected By
	
	Signature
	

	Account
	
	Contractor(s)
	

	In-Person or Remote?
	
	Adequate Evidence seen?
	

	Role
	
	Date & Time
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