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WORKING AT HEIGHT PERMIT
Copy of this permit shall be maintained in the immediate area of the work
(Electronic version may apply)
The permit to work at height is issued when the employee's feet are above the maximum height limit of 2 metres from the ground or a safe reference base (with the exception of the safe use of a ladder)
	Section A – DETAILS OF THE ACTIVITY								

	Company performing work
	
	RAMS/JSA Reference No.
	


	Works Location
	
	
	

	Works Description
	




	Client / Organization Notification

	Has the Client / Organization been notified of the work to be carried out? YES □  NO □
	Notified by (name): ____________________________
Date / Time: ____________________________

	Section B – EQUIPMENT / AREAS USED / ACCESSED	

	The following equipment/areas will be used/accessed to carry out the activity
	☐ Metal ladder
	☐ Roof

	☐ Movable metal scaffolding
	☐ Works near unprotected technological gaps

	☐ Fixed metal scaffolding
	☐ Other type of scaffolds (describe):

	☐ Mobile Elevated Working Platform (MEWP)
☐ Scaffolding tag (green/yellow/red) checked
☐ Weather conditions adequate (wind speed < safe limit)
	☐ Pillars
☐ Equipment/Machines
☐ Anchor points / Lifeline system in place
☐ Fall arrest system inspected and certified
☐ MEWP operator license verified

	☐ Other:
	




	Section C – PRECAUTIONS BEFORE STARTING THE ACTIVITY

	Have employees read and signed the risk assessment? YES / NO

	First Aider Assigned to this Work

	Is a First Aider assigned to this work?  YES □  NO □
	If YES – Name: ____________________________
Contact number: ________________________

	Visual inspection of the equipment used does not show any defects, improvisations, or missing elements.
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Will work be done on the roof at least 2 meters from the edge of the building?

	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Mandatory W@H checklist items:

	Edge protection verified (rails, toe boards, barriers)
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Ladder inspected and secured at top & bottom
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Rescue plan defined and available
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Weather conditions acceptable: wind < ___ km/h, no storms
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Area below activity cordoned off
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Tools secured against falling (lanyards, tool belts)
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Fragile roof access controlled
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	“Toolbox Talk conducted before starting work”
	YES ☐ NO ☐
	IF answer is NO, prevention measure must be added here:

	Personal protective equipment:
	☐ Safety shoes
	☐ Safety helmet

	☐ Protective harness
☐ Other PPE:
	☐ High vis vest/clothing






	
General precautions:
- The skylights, the domes, the lighting strips on the roof, the windows of the roofs have no mechanical retention capacity against void.                                                                                                                                                                                                                        - It is forbidden to step on hatches or windows or to use them as storage for tools and work equipment.
- In the case of carrying out work on roofs, as well as on skylights or roofs in the staircase, safety measures will be taken to prevent falling from height (e.g. the use of anchor points/lifeline systems and harnesses, retention nets, etc.).
- In the case of long-term works on installations, on the construction of new installations, site works, falling from height preventive measures will always be provided at the workplace.

	Dynamic Risk Assessment

	Hazards related to the work
	Preventive measures

	






	

	Section D – AUTHORIZATION AND VALIDITY

	Issued date: __________________Time: _________________ Expiration date: ________________ Time: ____________

Permit Issuer: _________________________________ Department________________Signature__________________

Permit Receiver: _______________________________Company___________________Signature__________________


	Section E – APPROVAL OF THE WORK - PERSONS INVOLVED
I/We have read and understood the dangers of this activity and undertake to adopt the previously mentioned preventive measures. 
I will stop the activity the moment I identify an imminent risk of injury. The defined measures are implemented at the site of the intervention and are checked.

	Section F – JOB COMPLETION/PERMIT EXPIRATION/PERMIT CLOSURE

	☐ I confirm that all works associated with this Work at Height Permit have been completed / not completed (strike through as applicable).
☐ All personnel have exited the Work at Height area and have safely returned to ground level.
☐ All tools, materials, and equipment have been removed from the work area and safely lowered to the ground.
☐ All fall protection equipment (harnesses, lanyards, anchor points, lifelines, retractables, etc.) has been removed, inspected after use, and stored correctly.
☐ All temporary edge protection, barriers, warning signs, exclusion zones, and access controls used during the activity have been restored to their original, safe condition.
☐ The work area has been inspected and is left in a safe condition with no remaining hazards.
☐ (If applicable) Any damage to the structure, roof, anchor points, or equipment has been reported to the Permit Issuer.
☐ (If work is incomplete) An extension request has been submitted before the expiry of this permit. If extension is not granted, a new permit must be issued prior to resuming work.

	Permit Issuer: ___________________________ Company ___________________________Signature________________
Permit Receiver: _________________________Company ___________________________Signature________________
Date: _____________
Hour: _____________
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